Run *.exe to start a standalone windows GUI for iCSA family of drivers.
A default *.iip project and *.LUT compensation file are included.

Run the .exe and select the project file.
Connect at the prompt and select file with the frequency range appropriate to iCSA- model variant  